/*******************************************************************************/
/** USB Driver
 *
 * version 3.3.0.0
 *
 * Copyright (C) 2020, OPTOELECTRONICS CO., LTD. All rights reserved.
 *******************************************************************************/


[Condition]
 - Required Microsoft .NET Framework 4.6

[Operating System]
 - Windows10 (32bit/64bit)
 - Windows8 / 8.1 (32bit/64bit)
 - Windows7 (32bit/64bit)

 - Windows 10 IoT Enterprise LTSB 2016 / LTSC 2019 (64bit)
 - Windows Embedded 8.1 Industry (32bit)
 - Windows Embedded POS Ready7 (32bit)

[Installation]
 1. Run Installer.exe (*1, *2) and select "Next".
 2. Select "Install" or "Uninstall".
 3. Select "OK" and finish.

*1:Run as administrator permission.
*2:Run before device connection (COM open).

[Command line options]
 /s : silent mode
 /u : uninstallation
 /r : reboot

[Usage]
 "Installer.exe /s"

 ExitCode returns 0 for normal completion.

[Reference sample]
 - SilentInstallSample.bat
